\section{marlintpc\-:\-:Test\-T\-P\-C\-Distortions\-Map\-Processor Class Reference}
\label{classmarlintpc_1_1TestTPCDistortionsMapProcessor}\index{marlintpc\-::\-Test\-T\-P\-C\-Distortions\-Map\-Processor@{marlintpc\-::\-Test\-T\-P\-C\-Distortions\-Map\-Processor}}


Processor skeleton for M\-A\-R\-L\-I\-N.  




{\ttfamily \#include $<$Test\-T\-P\-C\-Distortions\-Map\-Processor.\-h$>$}

Inheritance diagram for marlintpc\-:\-:Test\-T\-P\-C\-Distortions\-Map\-Processor\-:\begin{figure}[H]
\begin{center}
\leavevmode
\includegraphics[height=2.000000cm]{classmarlintpc_1_1TestTPCDistortionsMapProcessor}
\end{center}
\end{figure}
\subsection*{Public Member Functions}
\begin{DoxyCompactItemize}
\item 
virtual Processor $\ast$ {\bfseries new\-Processor} ()\label{classmarlintpc_1_1TestTPCDistortionsMapProcessor_a6b1c9efccd5c136f38acd024ba6ab1d1}

\item 
virtual void {\bfseries init} ()\label{classmarlintpc_1_1TestTPCDistortionsMapProcessor_a9193827aab8c01890e350f40d4b370e8}

\item 
virtual void {\bfseries process\-Run\-Header} (lcio\-::\-L\-C\-Run\-Header $\ast$run)\label{classmarlintpc_1_1TestTPCDistortionsMapProcessor_a12527508bc64ea75d0e634c66ffd378d}

\item 
virtual void {\bfseries process\-Event} (lcio\-::\-L\-C\-Event $\ast$evt)\label{classmarlintpc_1_1TestTPCDistortionsMapProcessor_ac6bfc82c884198ee78156e79168324ca}

\item 
virtual void {\bfseries check} (lcio\-::\-L\-C\-Event $\ast$evt)\label{classmarlintpc_1_1TestTPCDistortionsMapProcessor_a39d675620f82f92864b7ac0c5e47caf1}

\item 
virtual void {\bfseries end} ()\label{classmarlintpc_1_1TestTPCDistortionsMapProcessor_ac65afb26f0bb28d4b2f340a4bc0e1802}

\end{DoxyCompactItemize}


\subsection{Detailed Description}
Processor skeleton for M\-A\-R\-L\-I\-N. 

\begin{DoxyAuthor}{Author}
Ch. Rosemann, D\-E\-S\-Y 

M. Killenberg, C\-E\-R\-N
\end{DoxyAuthor}
Concrete implementation\-: \begin{DoxyAuthor}{Author}
K. Zenker, D\-E\-S\-Y
\end{DoxyAuthor}
This processor can be used to visualize the field distortions measured with system of photodots on the T\-P\-C cathode. They are stored in a conditions object (T\-P\-C\-Distortion\-Measurement) in the data base. Up to now arrows are drawn that point from the true photodot position on the cathode to the reconstructed position on the pad plane. 

The documentation for this class was generated from the following files\-:\begin{DoxyCompactItemize}
\item 
Test\-T\-P\-C\-Distortions\-Map\-Processor.\-h\item 
Test\-T\-P\-C\-Distortions\-Map\-Processor.\-cc\end{DoxyCompactItemize}
