
\begin{DoxyRefList}
\item[\label{todo__todo000018}%
Class \doxyref{Hep\-Rep\-Output\-Processor}{p.}{classHepRepOutputProcessor} ]Color or pattern coding of the quality flags should be implemented for the pads. 

not yet implemented, shall vary between a given color and \char`\"{}black\char`\"{} \begin{DoxyItemize}
\item C\-O\-L\-O\-R\-W\-H\-I\-T\-E = 6, \end{DoxyItemize}
not yet implemented, shall bleach a given color to \char`\"{}white\char`\"{} 
\begin{DoxyParams}{Parameters}
{\em Color} & -\/ \\
\hline
\end{DoxyParams}
not yet implemented, will be needed for some future color schemes.

not yet implemented shall become a nicer implemetation of a red blue scale. \begin{DoxyItemize}
\item C\-O\-L\-O\-R\-B\-R\-I\-G\-H\-T\-N\-E\-S\-S = 5, \end{DoxyItemize}

\item[\label{todo__todo000003}%
Class \doxyref{marlintpc\-:\-:Drift\-Processor}{p.}{classmarlintpc_1_1DriftProcessor} ]Implement full curler handling (10 electrons per hit for low p\-\_\-t and low p\-\_\-z) 
\item[\label{todo__todo000008}%
Class \doxyref{marlintpc\-:\-:Electron\-Cloud\-Finder\-Processor}{p.}{classmarlintpc_1_1ElectronCloudFinderProcessor} ]Implement calculation of z-\/coordinate by drift velocity 

Improve z cut. Currently it does not use topological information which can cause problems with curlers.

Handling of dead and noisy channels.  
\item[\label{todo__todo000004}%
Class \doxyref{marlintpc\-:\-:Hit\-Candidate}{p.}{classmarlintpc_1_1HitCandidate} ]F\-I\-X\-M\-E\-: Calculation of covariance matrix is missing, currently is unity. It should be the estimated error of the coordinates, not the varianve of the charge distribution.  
\item[\label{todo__todo000005}%
Member \doxyref{marlintpc\-:\-:Hit\-Candidate\-:\-:is\-At\-Boundary}{p.}{classmarlintpc_1_1HitCandidate_a37ff327241ec82938e9ec7768547106a} () const ]F\-I\-X\-M\-E\-: Calculation of boudary condition should be done automatically when adding a pulse  
\item[\label{todo__todo000006}%
Class \doxyref{marlintpc\-:\-:Hit\-Track\-Finder\-Topo\-Processor}{p.}{classmarlintpc_1_1HitTrackFinderTopoProcessor} ]Handling of dead and noisy channels. 

Improve z cut. Currently it does not use topological information which can cause problems with curlers. 
\item[\label{todo__todo000001}%
Class \doxyref{marlintpc\-:\-:Linear\-Geometric\-Mean\-Resolution\-Processor}{p.}{classmarlintpc_1_1LinearGeometricMeanResolutionProcessor} ]Currently only the histograms are filled. The resolution propper has to be calculated manually. 
\item[\label{todo__todo000002}%
Class \doxyref{marlintpc\-:\-:Linear\-Three\-Point\-Resolution\-Processor}{p.}{classmarlintpc_1_1LinearThreePointResolutionProcessor} ]Currently only the histogram is filled. The resolution propper has to be calculated manually. 
\item[\label{todo__todo000020}%
Member \doxyref{marlintpc\-:\-:Pulse\-Finder\-Tester\-:\-:run\-All\-Tests}{p.}{classmarlintpc_1_1PulseFinderTester_ac30d8efd994980b0331bff52ab9d6df8} ()]\-: Pulse\-Finder\-Tester\-: calculate correct time error and test it 

\-: Pulse\-Finder\-Tester\-: calculate correct charge error and test it 

\-: Pulse\-Finder\-Tester\-: calculate expected charge fit value and test it  
\item[\label{todo__todo000010}%
Class \doxyref{marlintpc\-:\-:Row\-Based\-Fast\-Hough\-Transformation\-Processor}{p.}{classmarlintpc_1_1RowBasedFastHoughTransformationProcessor} ]
\begin{DoxyItemize}
\item (average) track direction different from X direction ?
\item hit cleaning for segment creation ?
\item replace hard coded radial row number for timepix data ? 
\end{DoxyItemize}
\item[\label{todo__todo000007}%
Class \doxyref{marlintpc\-:\-:Row\-Based\-Hit\-Finder\-Processor}{p.}{classmarlintpc_1_1RowBasedHitFinderProcessor} ]Hit quality flag (including inheritance of pulse flags) 

Handling of dead and noisy channels. 
\item[\label{todo__todo000011}%
Class \doxyref{marlintpc\-:\-:Row\-Triplet\-Based\-Track\-Finder\-Processor}{p.}{classmarlintpc_1_1RowTripletBasedTrackFinderProcessor} ]
\begin{DoxyItemize}
\item definition of module neighbourhood from P\-O\-L\-A\-R module extend ?
\item better resolve equivalent (indirectly matching) overlapping segments ? 
\end{DoxyItemize}
\item[\label{todo__todo000012}%
Class \doxyref{marlintpc\-:\-:Simple\-Helix\-General\-Broken\-Line\-Interface\-Processor}{p.}{classmarlintpc_1_1SimpleHelixGeneralBrokenLineInterfaceProcessor} ]
\begin{DoxyItemize}
\item implement additional output of pull distributions, residuals, track paramters for each measurement point 
\end{DoxyItemize}
\item[\label{todo__todo000013}%
Class \doxyref{marlintpc\-:\-:Step\-Wise\-Helix\-General\-Broken\-Line\-Interface\-Processor}{p.}{classmarlintpc_1_1StepWiseHelixGeneralBrokenLineInterfaceProcessor} ]
\begin{DoxyItemize}
\item implement additional output of pull distributions, residuals, track paramters for each measurement point 
\end{DoxyItemize}
\item[\label{todo__todo000014}%
Class \doxyref{marlintpc\-:\-:Time\-Pix\-Local\-Road\-Search\-Processor}{p.}{classmarlintpc_1_1TimePixLocalRoadSearchProcessor} ]
\begin{DoxyItemize}
\item variable octoboard to (mechanical) module mapping (from G\-E\-A\-R file?) 
\end{DoxyItemize}
\item[\label{todo__todo000015}%
Member \doxyref{marlintpc\-:\-:Track\-Fitter\-Likelihood\-Processor\-:\-:Up}{p.}{classmarlintpc_1_1TrackFitterLikelihoodProcessor_a3d4e96e05c27d6941da054a8ea12f375} () const ]Comment a little bit better with links!!!!!!!!!!!!!!!!! Idem for error\-Def()  
\item[\label{todo__todo000016}%
Class \doxyref{marlintpc\-:\-:Track\-Fitter\-Simple\-Chi\-Square\-Pads}{p.}{classmarlintpc_1_1TrackFitterSimpleChiSquarePads} ]\-: Implement the fitter function. 
\end{DoxyRefList}