\section{I\-M\-P\-L Namespace Reference}
\label{namespaceIMPL}\index{I\-M\-P\-L@{I\-M\-P\-L}}


======= \doxyref{F\-P\-C\-C\-D\-Data}{p.}{classFPCCDData} ========== \par
 A class to store all F\-P\-C\-C\-D's data.  




\subsection{Detailed Description}
======= \doxyref{F\-P\-C\-C\-D\-Data}{p.}{classFPCCDData} ========== \par
 A class to store all F\-P\-C\-C\-D's data. \par
 Used by F\-P\-C\-C\-D\-Digitizer and F\-P\-C\-C\-D\-Clustering

pack\-Pixel\-Hits(...) copies Pixel\-Hit data in \-\_\-px\-Hits(\-Pixel\-Data\-Buf\-\_\-t) to L\-C\-Generic\-Object of name V\-T\-X\-Pixel\-Hits as integer data and unpack\-Pixel\-Hits(...) copies L\-C\-Generic\-Object to \-\_\-px\-Hits.

Format of L\-C\-Generic\-Object is as follows\-: Pixel\-Hits in one ladder are packed in one element.
\begin{DoxyItemize}
\item First 32 bit word contains layer\-I\-D and ladder\-I\-D of the element. Counting bit position from left to right, layer\-I\-D and ladder\-I\-D information are stored as follows. bit 31-\/16\-: reserved for future use bit 15-\/8 \-: layer\-I\-D bit 7-\/0 \-: ladder\-I\-D
\item Last words are for pixel hits in a ladder. Two word is used for each pixel hit. -- First word bit 31\-: 0 bit 30-\/29 \-: hit quality bit 0 = hit is created by a single Sim\-Tracker\-Hit of a signal event. 1 = hit is created by multiple Sim\-Tracker\-Hits of a signal event 2 = hit is created by a sigle Sim\-Tracker\-Hit of a signal event and hits by background events 3 = hit is created by multiple Sim\-Tracker\-Hits of a signal event and background events. bit 28-\/16 \-: xi\-I\-D bit 15-\/0 \-: zeta\-I\-D -- Second word d\-Edx value given by Sim\-Tracker\-Hit object. Float value is stored with a help of union.
\end{DoxyItemize}

\par
 \begin{DoxyAuthor}{Author}
Akiya Miyamoto, K\-E\-K\-: 2010-\/04-\/19 
\end{DoxyAuthor}
