\section{gear\-:\-:F\-T\-D\-Parameters Class Reference}
\label{classgear_1_1FTDParameters}\index{gear\-::\-F\-T\-D\-Parameters@{gear\-::\-F\-T\-D\-Parameters}}


Geometry properties of a F\-T\-D detector needed for reconstruction code.  




{\ttfamily \#include $<$F\-T\-D\-Parameters.\-h$>$}

Inheritance diagram for gear\-:\-:F\-T\-D\-Parameters\-:\begin{figure}[H]
\begin{center}
\leavevmode
\includegraphics[height=3.000000cm]{classgear_1_1FTDParameters}
\end{center}
\end{figure}
\subsection*{Public Member Functions}
\begin{DoxyCompactItemize}
\item 
virtual {\bf $\sim$\-F\-T\-D\-Parameters} ()\label{classgear_1_1FTDParameters_aba1516491968cb80d90bef96b88a558a}

\begin{DoxyCompactList}\small\item\em Destructor. \end{DoxyCompactList}\item 
virtual const {\bf F\-T\-D\-Layer\-Layout} \& {\bf get\-F\-T\-D\-Layer\-Layout} () const =0\label{classgear_1_1FTDParameters_a450b9b04c153aeae5500554825c22ec0}

\begin{DoxyCompactList}\small\item\em The layer layout in the Vertex. \end{DoxyCompactList}\end{DoxyCompactItemize}
\subsection*{Static Public Attributes}
\begin{DoxyCompactItemize}
\item 
static const int {\bfseries P\-I\-X\-E\-L} = 1\label{classgear_1_1FTDParameters_a255d354c6afba9456cc680cb498d7082}

\item 
static const int {\bfseries S\-T\-R\-I\-P} = 2\label{classgear_1_1FTDParameters_a784e86fb6a362baad05b060d9bb46f27}

\item 
static const int {\bfseries F\-A\-C\-E} = 1\label{classgear_1_1FTDParameters_a71c15c9ddce4fa97ef039d7e7e5c9c9a}

\item 
static const int {\bfseries B\-A\-C\-K} = 2\label{classgear_1_1FTDParameters_a2b45fd6cba47a60e46a8eebf7a8258a8}

\end{DoxyCompactItemize}


\subsection{Detailed Description}
Geometry properties of a F\-T\-D detector needed for reconstruction code. 

\par
 

The F\-T\-D is assumed to consist of a number of disks (layers) located along the Z-\/axis. Each disk consists of a number of trapezoid ladders (petals) that are uniformly distributed in a circle around the Z-\/axis .\par
 The sensitive volumes are rectangular pixels for the disks 1 and 2 covering the petal face nearest the I\-P; the remaining disks mount trapezoids covering both faces of the petal (we assume 1 sensitive layer per face; in the current implementation there are two). The sensitive volumes can be placed relative to the (insensitive) ladders. \begin{DoxySeeAlso}{See Also}
add\-Layer .
\end{DoxySeeAlso}
N\-B\-: The \doxyref{F\-T\-D\-Parameters}{p.}{classgear_1_1FTDParameters} describe the one half of the detector at the positive z-\/axis and the other half of the detector is built as a reflection in the X\-Y-\/plane.\par


\begin{DoxyAuthor}{Author}
J. Duarte; I\-F\-C\-A (based from V\-X\-D\-Parameters\-Impl) 
\end{DoxyAuthor}
\begin{DoxyVersion}{Version}
\$\-Id\-: 
\end{DoxyVersion}


Definition at line 29 of file F\-T\-D\-Parameters.\-h.



The documentation for this class was generated from the following file\-:\begin{DoxyCompactItemize}
\item 
F\-T\-D\-Parameters.\-h\end{DoxyCompactItemize}
